FS28_Bluetooth_Slave_Mode_Demo_v1.4.exe is the tools for controlling FS28 in slave Mode. Password is need to run these tools. The default password is 123456
FS28_Bluetooth_Slave_Mode_Demo_v1.4.exe is only compatible with FS28 with AVR firmware version V5.2.3 or above.